08/01/2014

S609-14.docx

|  |
| --- |
| Use on projects as appropriate. |

## Section 609. — CURB AND GUTTER

**Description**

**609.01** Add the following:

This work also consists of constructing paved ditches along the roadway.

|  |
| --- |
| When constructing paved asphalt ditches include 609.03 below and 609.08A.. |

**Construction Requirements**

**609.03 General.** Add the following:

For asphalt paved ditches, form the bed parallel to the finished surface of the ditch.

|  |
| --- |
| When gluing concrete curb to asphalt pavement, insert 609.03 below. |

**609.03 General.** Add the following:

When bonding concrete curb to existing asphalt pavement thoroughly clean the pavement surface in advance of placing the curb. Abrade and/or high pressure water wash the existing asphalt pavement to assure removal of all dust and loose material.

Bond the extruded curb or precast curb to the existing asphalt pavement using an approved concrete to asphalt adhesive or a two-component epoxy, designed to bond fresh concrete to the existing pavement. Submit proposed adhesive for approval by the CO prior to use. Apply according to the manufacturer’s recommendations.

|  |
| --- |
| Use 609.08A on all projects with asphalt paved ditches and 609.03 above. |

Add the following:

**609.08A Asphalt Paved Ditch.** Perform the work according to Section 403, Type II. Before overlaying existing asphalt paved ditches, clean and seal the cracks according to Section 414. Compact according to Subsection 403.09.

|  |
| --- |
| Use on all projects with curbing and/or ditches. |

**Measurement**

**609.10** Add the following:

When measuring paved ditches, measure the length along the face of the curb.

No separate measurement will be made for the asphalt mixture included in asphalt curb or paved ditch.