## Section 251. — RIPRAP

11/05/15– FP-14

Construction Requirements

WFL Specification 01/01/14 2510010

Include the following when there is limited vertical clearance to work (i.e. under bridges, in box culverts).

Edit as required for non-bridge work.

### 251.03 General.

Add the following:

Place riprap under or adjacent to structures before placing prefabricated superstructure units or constructing superstructure falsework.