## Section 553. — PRESTRESSED CONCRETE

7/21/17–FP14

WFL Specification 7/21/17 5530010

Include the following in all projects that require prestressed concrete.

Material

### 553.02

 Add the following to the material list:

Non-shrink grout 725.13(b)

Construction Requirements

### 553.03 Qualifications.

Delete paragraph (a).

### 553.09 Storing, Transporting, and Erecting.

Delete the second paragraph and substitute the following:

Before transporting prestressed concrete members, provide written certification from the precast concrete manufacturing plant Quality Control Manager that the members were fabricated and inspected according to the contract and meet minimum quality requirements.