##  Section 603. — STRUCTURAL PLATE STRUCTURES

07/20/15–FP14

Construction Requirements

FLH Transmittal No. 1 7/20/15 6030010

Include the following on all projects that require work in this Section.

### 603.04 Erecting.

Delete the seventh paragraph and substitute the following:

Torque steel bolts and aluminum bolts on 0.1-inch (2.5-millimeter) thick and heavier aluminum plates to at least 115 foot-pounds (155 newton-meters) and a maximum of 130 foot-pounds (180 newton-meters).