## Section 625. — TURF ESTABLISHMENT

08/01/14–FP14

Construction Requirements

WFL Specification 08/01/14 6250010

Include the following when work is required under this Section.

### 625.03 General.

Delete the text of this Subsection and substitute the following:

Apply turf establishment to finished slopes and ditches between [INSERT DATE] and [INSERT DATE]. Do not apply turf establishment during windy weather or when the ground is excessively wet, frozen, snow covered, extremely dry, cloddy, hard pan, or not friable.

WFL Specification 08/01/14 6250020

Include the following when limestone is required.

### 625.04 Preparing Seedbed.

Add the following:

Apply agricultural limestone at the rate of [INSERT #] pounds per acre ([INSERT #] kilograms per hectare).

WFL Specification 08/01/14 6250030

Include the following when water is not required.

 Note: If water is required include pay item in EE.

### 625.05 Watering.

Delete the text of this Subsection.

WFL Specification 08/01/14 6250040

Include the following when fertilizing by hydraulic method is required.

### 625.06 Fertilizing.

Add the following to paragraph (b):

Apply fertilizer at the rate of [INSERT #] pounds (kilograms) per slurry unit. Fertilize areas inaccessible to hydraulic-type equipment by hand.

WFL Specification 08/01/14 6250050

Include the following when seeding by hydraulic method is required.

 Note: List seed mix in Subsection 713.04.

### 625.07 Seeding.

Add the following to paragraph (b):

Apply the seed at the rate of [INSERT #] pounds (kilograms) of live seed per [INSERT ACRE (HECTARE) or SLURRY UNIT].

WFL Specification 08/01/14 6250060

Include the following when mulching by hydraulic method is required.

 Note: add alternative mulches if acceptable.

### 625.08 Mulching.

Delete the second and third paragraphs of paragraph (b) and substitute the following:

Apply [INSERT MULCH DESCRIPTION] at a rate of [INSERT #] pounds (kilograms) per [INSERT ACRE (HECTARE) OR SLURRY UNIT] upon completion of seeding and fertilizing applications. This rate does not apply to mulch for tracer applied under Subsection 625.07 (b), Seeding, Hydraulic Method.