## Section 633. — PERMANENT TRAFFIC CONTROL

08/01/14–FP14

Construction Requirements

WFL Specification 08/01/14 6330010

Include the following when specific sign post material is required.

Note: Post installation details for each type of post material chosen will be required in the contract. (Reference to other State DOT post installation details may be used if there are no conflicts with the contract documents.)

### 633.04 Sign Posts.

Add the following:

Fabricate sign posts from [INSERT wood, aluminum, galvanized steel, or corrosion resistant steel or combination thereof].

WFL Specification 08/01/14 6330020

Include the following when sign panel fabrication is required.

### 633.05(a)(1) Panels.

Amend as follows

Delete the sixth paragraph and substitute the following:

Use retroreflective sheeting as specified and according to ASTM D4956. For roadside signs, use Type III, IV, VIII, IX, or XI prismatic retroreflective sheeting. Use fluorescent yellow-green sheeting for school crossing signs.

WFL Specification 08/01/14 6330030

Include the following when specific sign panel material is required.

Add the following:

Fabricate sign panels from [INSERT plywood, aluminum, steel, plastic, or fiberglass reinforced plastic].