## Section 719. — PAINT

06/15/22–FP14

WFL Specification 06/15/22 7190005

Include the following when bridge painting is required. Consult with Bridge for color numbers.

719.04 Paint for Steel Structures.

Add the following to the first paragraph:

Top coat color to match AMD-STD [INSERT COLOR NUMBER] for [INSERT BRIDGE NAME] Bridge for girder ends and steel members.

Top coat color to match AMS-STD [INSERT COLOR NUMBER] for [INSERT BRIDGE NAME] Bridge rail.

WFL Specification 08/01/14 7190010

Include the following when Section 613 is required.

### 719.08 Penetrating Stain.

Delete the last sentence and add the following:

**(e) Mildew resistance:** According to Federal Test Method Standard 144, Method 6271.

Store stain according to manufacturer's recommendations, with special attention given to recommended temperature range.