08/01/2014

S258-14.docx

|  |
| --- |
| Use on all projects with reinforced concrete retaining walls |

## Section 258. – REINFORCED CONCRETE RETAINING WALLS

**Materials**

**258.02** Add the following:

Geocomposite sheet drain 714.02(b)

**Measurement**

**258.08** Delete the second paragraph and substitute the following:

For concrete retaining wall, determine the square foot area from the length of wall along gutterline at top of finished roadway and the height excluding footings.

Delete the third paragraph and substitute the following:

Do not measure the following for payment: structure excavation (walls), backfill material, wall backfill, foundation fill, structural backfill, structural concrete, reinforcing steel, epoxy coated reinforcing steel, joint material, geocomposite sheet drain, perforated pipe, outlet pipe, and shoring and bracing.

**Payment**

**258.09** Add the following:

Payment for reinforced concrete retaining wall will be made under the reinforced concrete retaining wall item contained in the bid schedule which corresponds to the actual constructed height. For constructed wall heights that fall between two bid item heights, payment will be made under the pay item which most nearly describes the actual height. (For example, walls measuring 6.99 feet in height will be paid as a 6 foot wall, and walls measuring 7.00 feet in height will be paid as an 8 foot wall.)