## Section 258. — REINFORCED CONCRETE RETAINING WALLS

09/17/18– FP-14

Construction Requirements

WFL Specification 09/17/18 2580010

Include the following when both of the following conditions are met:

Work is done under this Section, and;

A pay item exists for structural excavation or backfill as part of this work.

### 258.03 General.

Delete the second paragraph and substitute the following:

Perform the work under Section 208.

### 258.06 Backfilling.

Delete the text of the first paragraph and substitute the following:

Backfill the area behind the wall with structural backfill according to Subsection 208.09. Compact each layer according to Subsection 208.10 using an approved lightweight mechanical, or vibratory compactor within 36 inches (900 millimeters) of the wall.

### 258.07 Acceptance.

Delete the third paragraph and substitute the following:

Structure excavation and backfill will be evaluated under Section 208.

Measurement

### 258.08

Add the following:

Measure structural excavation and backfill under Section 208.