## Section 617. — GUARDRAIL

11/12/20–FP14

WFL Specification 11/12/20 6170001

Include the following when weathering agent is required on galvanized steel guardrail components.

Material

### 617.02

Add the following:

Painting 563

Construction Requirements

WFL Specification11/12/20 6170005

Include the following when weathering agent is required on galvanized steel guardrail components.

### 617.03 General.

Add the following:

Apply weathering agent to all galvanized steel guardrail system and terminal section components according to Section 563.

WFL Specification 08/01/14 6170010

Include the following when alternate hole arrangements are required.

Note: Use for future pavement overlays. Insert 617-10 for wood posts and 617-11 for steel posts.

### 617.04 Post Installation.

Add the following:

Use alternate hole arrangement detail as shown on Standard 617-[INSERT #].

WFL Specification 11/12/20 617020

Include the following when weathering agent is required on galvanized steel guardrail components.

### 617.11 Acceptance.

Add the following:

Painting will be evaluated under Section 563.