## Section 635. — TEMPORARY TRAFFIC CONTROL

11/12/20–FP14

WFL Specification 01/01/14 6350010

Include the following when a Traffic Control Supervisor is required.

### Description

### 635.01

Add the following:

This work also includes providing the services of a Traffic Control Supervisor.

WFL Specification 10/31/16 6350020

Include the following when work is required under this Section.

Material

### 635.02

Amend as follows:

Delete the following from the material list:

Sign panels 633.05

Sign posts 633.04

Add the following to the material list:

Sign hardware 718.06

Sign panels 718.03

Sign posts 718.04

Construction Requirements

WFL Specification 10/31/16 6350030

Include the following when work is required under this Section.

### 635.07 Construction Signs.

Delete the text of this Subsection and substitute the following:

Fabricate and install sign panels according to Subsection 633.05. Use Type III, IV, VIII, IX, or XI prismatic retroreflective sheeting on sign panels. Roll-up signs may be used instead of panels when approved by the CO. For roll-up signs, use Type VI retroreflective sheeting.

Furnish posts conforming to Subsection 718.04, except wood posts may be untreated. Install posts according to Subsection 633.04. Portable sign supports may be used instead of sign posts when approved by the CO.

Remove or completely cover unnecessary signs. Use metal, plywood, or other acceptable material to cover signs. Do not use adhesive glue, tape, or mechanical fasteners that mar the face of the panel of the sign to be covered.

WFL Specification 01/01/14 6350040

Include the following when a Traffic Control Supervisor is required.

### 635.08A Traffic Control Supervisor.

(Added Subsection).

Perform services described in Subsection 156.09. Provide all vehicles and incidentals necessary to perform the work.

WFL Specification 06/17/14 6350050

Include the following when temporary pavement markings and delineation is required on the final alignment before permanent markings are applied. Not appropriate for use when project staging requires interim markings that are different than those needed for the final alignment.

Note: Use when paving will last more than one day.

### 635.13 Temporary Pavement Markings and Delineation.

Add the following after the first paragraph:

Apply temporary pavement markings to the same locations and cycle lengths as shown in the plans for permanent pavement markings, including all passing zones.

WFL Specification 11/12/20 6350060

Include the following when temporary pavement markings are required. Edit as required.

### 635.13A Temporary Signs and Vehicle Positioning Guides.

(Added Subsection).

Temporary signs and vehicle positioning guides may be substituted for temporary pavement markings for up to 14 calendar days. Install “NO CENTER LINE” (W8-12), “NO PASSING ZONE” (W14-3), “DO NOT PASS” (R4-1) and “PASS WITH CARE” (R4-2) signs according to the MUTCD. Include the description and location of each sign in an alternate traffic control proposal according to Subsection 156.04. Install vehicle positioning guides (temporary raised pavement markers) spaced 40 feet (12 meters) apart for temporary centerline delineation.

WFL Specification 04/20/18 6350070

Include the following when work is required under this Section.

### 635.23 Acceptance.

Delete the first paragraph and substitute the following:

Material for temporary traffic control devices will be evaluated under Subsections 106.02 and 106.03. Do not provide a copy of the certifications for temporary traffic control materials to the CO, unless otherwise directed by the CO.

Measurement

### 635.24

Add the following:

Measure flaggers for each hour a person is actually flagging.

WFL Specification 06/17/14 6350080

Include the following when the Traffic Control Supervisor is a pay item measured by the DAY in the Bid Schedule.

Measure Traffic Control Supervisor by the day for the work described in Subsection 156.09.

A day will be measured when:

**(a)** Construction operations require a Traffic Control Supervisor during the normal working days;

**(b)** The Traffic Control Supervisor makes normal checks during nonwork hours; or

**(c)** The Traffic Control Supervisor is called out during nonwork hours.

Do not measure flagging performed by the Traffic Control Supervisor when there is a pay item in the bid schedule for Traffic Control Supervisor.

WFL Specification 01/01/14 6350090

Include the following when temporary pavement markings are required.

Add the following:

Signs used to delineate passing zones and raised pavement markers used for vehicle positioning guides according to Subsection 635.13A will not be measured.

Payment

WFL Specification 01/01/14 6350100

Include the following when an item for temporary pavement markings is in the bid schedule.

### 635.25.

Add the following:

Progress payment for temporary pavement markings will be made upon installation, except that when the pay item includes subsequent removal of the markings, up to 25 percent of the unit bid price may be withheld until the removal is completed.