06/13/2019

S301-14\_06132019.docx

|  |
| --- |
| Use on projects with **more** than 5000 tons (statistical acceptance). |

## Section 301. — UNTREATED AGGREGATE COURSES

**Construction Requirements**

**301.03 General.** Add the following:

For base course set target values within the gradation ranges shown in Table 703-2, grading C, D, or E.

For surface course aggregate set target values within the gradation range shown in Table 703-3.