*INCLUDE SECTION 156 ON ALL PROJECTS WITH THE FOLLOWING CLAUSES AS A MINIMUM:*

*- $$156.04A OR $$156.04B;*

*- $$156.08A OR $$156.08B; AND*

*- $$156.09A OR $$156.09B*

*REMOVE ITALICS, PARENTHESES, AND QUOTATION MARKS FROM INSERT FIELDS*

$$156.00A

Section 156. — PUBLIC TRAFFIC

Revised 22 June 2016

*INCLUDE THE FOLLOWING ON ALL PROJECTS EXCEPT WHEN REQUIRING THE CONTRACTOR TO SUBMIT A TRAFFIC CONTROL PLAN - IF THE CONTRACTOR IS REQUIRED TO SUBMIT A TRAFFIC CONTROL PLAN, USE CLAUSE $$156.04B INSTEAD (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.04B)*

$$156.04A

156.04. Delete the first paragraph and substitute the following:

Accommodate traffic according to the MUTCD, contract traffic control plan, Section 635, and this Section. An alternate traffic control plan may be submitted for approval in accordance with Subsection 104.03 and the following:

1. Ensure safe and efficient pedestrian, bicycle, and vehicular traffic (including emergency vehicles) at all times during construction;
2. Schedule and perform work to minimize disruption to public traffic; and
3. Accommodate the construction operations as approved under Section 155.

Submit alternate traffic control plans at least 30 days before its intended use. After the initial traffic control plan is approved, revise it as necessary to accommodate approved changes in the construction schedule. Submit the revised traffic control plan at least 14 days before implementation, unless otherwise approved by the CO.

*INCLUDE THE FOLLOWING IF THE CONTRACTOR IS REQUIRED TO SUBMIT A TRAFFIC CONTROL PLAN - EDIT CONTENT AS NEEDED - DO NOT INCLUDE THIS CLAUSE IF A TRAFFIC CONTROL PLAN IS PROVIDED (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.04A)*

$$156.04B

156.04. Delete the first paragraph and substitute the following:

Accommodate traffic according to the MUTCD, contract traffic control details, Section 635, and this Section. Submit a traffic control plan for approval at least 30 days before its intended use in accordance with Subsection 104.03 and the following:

1. Ensure safe and efficient pedestrian, bicycle, and vehicular traffic (including emergency vehicles) at all times during construction;
2. Schedule and perform work to minimize disruption to public traffic;
3. *(insert project specific traffic control requirements)*;
4. *(insert project specific traffic control requirements)*; and
5. Accommodate the construction operations as approved under Section 155.

Revise the traffic control plan as necessary to accommodate approved changes in the construction schedule. Submit the revised traffic control plan at least 14 days before implementation, unless otherwise approved by the CO.

*INCLUDE THE FOLLOWING IF ANY OF THE CLAUSES $$156.04D THRU $$156.04L ARE USED - VERIFY WITH PARTNER AGENCY IF CLAUSES ARE APPROPRIATE FOR THE PROJECT*

$$156.04C

156.04. Add the following:

*INCLUDE THE FOLLOWING IF APPLICABLE*

$$156.04D

Maintain one lane of traffic at all times.

*INCLUDE THE FOLLOWING IF USING SINGLE LANE CLOSURES*

$$156.04E

Use single lane closures on *(insert roadway name)* according to Section 635 and as shown in the plans.

*INCLUDE THE FOLLOWING FOR PROJECTS IF INSTALLATION OF TRAFFIC CONTROL DEVICES IS REQUIRED BEFORE BEGINNING WORK*

$$156.04F

Install *(insert devices)* according to Section 635 and as shown in the plans or as directed by the CO, at least *(insert minimum amount)* days before beginning work.

*INCLUDE THE FOLLOWING IF SPECIFYING A PERIOD WHEN ROADWAY CLOSURES ARE ALLOWED - DO NOT INCLUDE IF ROADWAY CLOSURES ARE ALLOWED THROUGHOUT THE DURATION OF THE PROJECT*

$$156.04G

*(Insert roadway name)* closures are permitted from *(insert specific date MM DD, YYYY)* to *(insert specific date MM DD, YYYY)*.

*INCLUDE THE FOLLOWING IF SPECIFYING A PERIOD WHEN ROADWAY CLOSURES ARE NOT ALLOWED*

$$156.04H

Do not close *(insert roadway name)* from *(insert specific date MM DD, YYYY)* to *(insert specific date MM DD, YYYY)*.

*INCLUDE THE FOLLOWING IF APPROVAL IS NEEDED FOR ROADWAY CLOSURES*

$$156.04I

Close *(insert roadway name)* to traffic during construction as approved by the CO. Open roadway within 24 hours after completion of work or as directed by CO.

*INCLUDE THE FOLLOWING IF A SPECIFIC ROADWAY CANNOT BE CLOSED THROUGHOUT THE DURATION OF THE PROJECT*

$$156.04J

Do not close *(insert roadway name)* to traffic during construction.

*INCLUDE THE FOLLOWING TO MAINTAIN ACCESS TO SPECIFIC ROADWAYS OR FACILITIES DURING CONSTRUCTION*

$$156.04K

Maintain access to *(insert roadways or facilities)* at all times.

*INCLUDE THE FOLLOWING FOR RUSH HOUR RESTRICTIONS ON PROJECTS WITH HIGH ADT OR IN URBAN AREAS - VERIFY WITH CONSTRUCTION IF PAYMENT REDUCTION AMOUNT IS ADEQUATE*

$$156.04L

Schedule and perform the work so it does not interfere with traffic during the rush hours shown in Table 156-1.

|  |
| --- |
| **Table 156-1****Rush Hours (Monday to Friday)** |
| **Morning** | #:## a.m. to #:## a.m. |
| **Evening** | #:## p.m. to #:## p.m. |

Do not install traffic control devices during the rush hours. Before rush hours begin, remove materials, equipment, and non-applicable traffic control devices from the roadway and install the necessary traffic control devices to safely maintain traffic. The CO reserves the right to review the Contractor’s progress before the rush hours begin. The CO may direct the Contractor to stop operations to ensure the Contractor completes all work, including the appropriate setup of traffic control devices, before the rush hours begin.

Failing to complete work and removing traffic control devices before a rush hour begins, or installing or removing them during rush hours will be considered Contractor noncompliance. Noncompliance will result in a reduction in payment to the Contractor equal to $(*insert amount*) per hour, for each hour or portion thereof. This reduction in payment will be subtracted from the Contractor’s progress payments and will be unrecoverable.

*INCLUDE THE FOLLOWING IF DRAINS OR INLETS ARE PRESENT WITHIN THE PROJECT LIMITS - VERIFY IF THE 157 INLET PROTECTION PAY ITEM IS NEEDED*

$$156.05A

156.05(f). Add the following:

Ensure that drains and inlets within the project limits are fully functional throughout the duration of the project.

*INCLUDE THE FOLLOWING IF PROVIDING A LANE WIDTH OF 10 FEET IS NOT POSSIBLE*

$$156.07A

156.07(c). Delete the first sentence.

Provide minimum lane widths of 9 feet.

*INCLUDE THE FOLLOWING TO SPECIFY THE LOCATION OF THE STAGING AREA - IF APPROVAL IS REQUIRED BEFORE THE CONTRACTOR CAN USE THE STAGING AREA, USE CLAUSE $$156.07C INSTEAD*

$$156.07B

156.07(d). Delete the first sentence and substitute the following:

Use *(insert location)* as a staging area.

*INCLUDE THE FOLLOWING TO SPECIFY THE LOCATION OF THE STAGING AREA AND APPROVAL IS REQUIRED BEFORE MOBILIZING INTO THE STAGING AREA*

$$156.07C

156.07(d). Delete the first sentence and substitute the following:

The Contractor may use *(insert location)* as a staging area. Obtain approval from the CO before using this location for staging.

*INCLUDE THE FOLLOWING IF STAGING IS PERMITTED OUTSIDE OF AREAS TO BE RECONSTRUCTED*

$$156.07D

156.07(d). Add the following:

Restore staging areas to their original condition as directed by CO.

*INCLUDE THE FOLLOWING FOR URBAN AREAS - REVISE ALLOWABLE DELAY AS NEEDED TO FIT PROJECT SPECIFIC NEEDS*

$$156.07E

156.07(i). Delete the Subsection and substitute the following:

1. Limit construction-caused delays to public traffic to a maximum of 15 minutes per passage through the project; and

*INCLUDE THE FOLLOWING FOR LIMITING THE LENGTH OF LANE CLOSURES*

$$156.07F

156.07. Add the following:

**(k)** Limit lane closures to *(insert maximum distance allowed)* feet unless otherwise approved by the CO.

*INCLUDE THE FOLLOWING IF NIGHTTIME OPERATIONS ARE NOT PERMITTED - VERIFY WITH PARTNER AGENCY AND CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSES $$156.08B, $$156.08C, AND $$156.08D)*

$$156.08A

156.08. Delete the second paragraph and substitute the following:

Nighttime operations are not permitted.

*INCLUDE THE FOLLOWING IF NIGHTTIME OPERATIONS ARE PERMITTED - VERIFY WITH PARTNER AGENCY AND CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT - VERIFY WITH CONSTRUCTION THE MINIMUM AMOUNT OF TIME NEEDED FOR THE REQUEST (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.08A)*

$$156.08B

156.08. Add the following:

Nighttime operations are permitted upon approval by the CO. Submit request to the CO for approval at least 3 days before any planned nighttime operations.

*INCLUDE THE FOLLOWING TO INDICATE ACTIVITIES THAT ARE NOT TO BE PERFORMED AT NIGHT - VERIFY WITH PARTNER AGENCY AND CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.08A)*

$$156.08C

Do not perform *(insert activities that the Contractor cannot perform at night)* work at night.

*INCLUDE THE FOLLOWING FOR REQUIRING SPECIFIC ACTIVITIES TO BE PERFORMED AT NIGHTTIME - VERIFY WITH PARTNER AGENCY AND CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT(IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.08A)*

$$156.08D

Perform *(insert activities that the Contractor is required to perform at night)* work at night.

*INCLUDE THE FOLLOWING FOR COMPLEX URBAN PROJECTS - VERIFY WITH CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.09B)*

$$156.09A

156.09. Add the following:

Provide a full-time traffic control supervisor exclusively for the project. Ensure the traffic control supervisor is on the site at all times when work is being performed and available during non-work periods.

*INCLUDE THE FOLLOWING FOR RURAL OR UNCOMPLICATED PROJECTS - VERIFY WITH CONSTRUCTION IF CLAUSE IS APPROPRIATE FOR THE PROJECT (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$156.09A)*

$$156.09B

156.09. Delete the second sentence and substitute the following:

The superintendent may serve as the traffic control supervisor provided the requirements of Subsection 156.03 are met.