*INCLUDE SECTION 609 ON PROJECTS WHERE PAY ITEM 60915-1000 CONCRETE WHEELSTOP IS USED OR WHEN DETAIL E609-02 IS USED*

$$609.00A

Section 609. — CURB AND GUTTER

Revised 12 February 2019

*INCLUDE CLAUSES $$609.02A, $$609.08A, AND $$609.09A FOR SEALANT AND GROUT APPLICATION FOR CONCRETE WHEESTOPS - VERIFY THE MATERIAL REFERENCES IN CLAUSE $$609.02A WITH MATERIALS ENGINEER AND REVISE ACCORDINGLY.*

$$609.02A

609.02. Add the following:

Grout 725.13(a)(2)

Sealant 712.01(a)(4)

$$609.08A

609.08. Add the following:

Place grout and sealant in the openings of the wheelstops as shown in the plans.

$$609.09A

609.09. Add the following:

Grout will be evaluated under Subsection 106.02.

Sealant will be evaluated under Subsection 106.02.