09/11/2014

S261-14\_09112014.docx

|  |
| --- |
| Use on all projects with reinforced soil slopes. (Verify actual pay items with geotech – CFL doesn’t use square foot face pay item for RSS). |

## Section 261. — REINFORCED SOIL SLOPES

**Measurement**

**261.07** Delete the second paragraph and add the following:

Measure earthwork under Section 204.

Measure reinforcement under Section 207.