*INCLUDE SECTION 154 ON ALL PROJECTS WITH CLAUSES $$154.02A, $$154.03A, AND $$154.03B AS A MINIMUM*

$$154.00A

Section 154. — CONTRACTOR SAMPLING AND TESTING

Revised 17 November 2020

*INCLUDE CLAUSES $$154.02A, $$154.03A, AND $$154.03B ON ALL PROJECTS*

$$154.02A

154.02. Add the following:

Submit proposals for using alternate AASHTO or state department of transportation approved test methods in writing for approval. Alternate methods may be allowed based on documented equivalence to the method specified and if approved by the CO.

$$154.03A

154.03. Add the following:

Provide the Government’s portion of the sample or split sample in an acceptable container suitable for shipment to the CO. The CO will sign and seal the sample with specialty chain-of-custody security tape. Ship the security-sealed sample to the EFLHD Central Laboratory at the following address within 24 hours of receiving the sample from the CO:

Federal Highway Administration

Eastern Federal Lands Highway Division

1827 Jack Delozier Drive

Sevierville, Tennessee 37876

ATTN: MATERIALS LABORATORY

$$154.03B

For the split sample of asphalt concrete pavement material, provide 5-gallon metal buckets with lids. As an alternative, provide boxes that are coated with silicone-coated paper throughout the interior.

*INCLUDE THE FOLLOWING IF MATERIAL IS BEING ACCEPTED UNDER SUBSECTION 106.05 STATISTICAL EVALUATION (USUALLY FOR THE FOLLOWING ITEMS: 258, 301, 309, 311, 314, 401, 402, 405, 407, 552, 565, 566, 568, AND 569 - SEE THE APPROPRIATE FP “ACCEPTANCE” SUBSECTION FOR THESE SECTIONS) (INCLUDE NO MATTER IF THE PAY ITEM QUANTITY QUALIFIES FOR A MATERIAL INCENTIVE OR NOT) (IF CLAUSE $$154.05A IS INCLUDED, ALSO INCLUDE CLAUSE $$106.05A)*

$$154.05A

154.05. Add the following:

For items accepted under Subsection 106.05, use the QL-PAY software program to determine pay factors and report pay factors determined by QL-PAY. Submit a copy of all current test results and pay factor calculations based on those tests on a weekly basis. When large quantities are produced, calculate pay factors as soon as possible. Use this information to make any necessary adjustments to operations to achieve acceptable pay factors. See Subsection 106.01 for conditions upon which the Government may use the Contractor’s test results.