*INCLUDE SECTION 203 ON ALL PROJECTS WITH EITHER CLAUSE $$203.05B OR $$203.05C AS A MINIMUM*

$$203.00A

**Section 203. — REMOVAL OF STRUCTURES AND OBSTRUCTIONS**

Revised 12 May 2016

*INCLUDE CLAUSES $$203.04A AND $$203.04B TO SPECIFY STRUCTURAL CONCRETE REMOVAL USING MECHANICAL IMPACT METHODS - VERIFY WITH BRIDGE IF CLAUSE IS APPROPRIATE TO USE - EDIT HAMMER IMPACT STRENGTH IF NECESSARY TO MEET PROJECT SPECIFIC NEEDS*

$$203.04A

203.04(c). Add the following after the second sentence of the first paragraph:

On structures, use power-driven hand tools and other hand tools in accordance with Subsection 203.04(e).

$$203.04B

203.04. Add the following:

1. **Concrete removal by mechanical impact methods.** Furnish equipment that complies with the following:
2. Use power-driven hand tools for removal of existing concrete with the following restrictions:
3. Do not use jackhammers heavier than 30 pounds;
4. Do not operate jackhammers and mechanical chipping tools at an angle in excess of 45 degrees measured from the surface of the concrete; and
5. Do not use chipping hammers heavier than a nominal 15-pound class to remove concrete from beneath any reinforcing bar.
6. Use hand tools (hammers and chisels) for removal of final particles of concrete or to achieve the required depth.

*INCLUDE THE FOLLOWING IF BURNING DEBRIS IS PROHIBITED - VERIFY WITH PARTNER AGENCY*

$$203.05A

203.05(b). Delete the Subsection and substitute the following:

1. **Burn.** Burning is prohibited.

*INCLUDE THE FOLLOWING IF BURYING DEBRIS IS ALLOWED - VERIFY WITH PARTNER AGENCY (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$203.05C)*

$$203.05B

203.05(c). Add the following after the first sentence of the first paragraph:

Bury debris beyond the toes of fills in areas authorized by the CO.

*INCLUDE THE FOLLOWING IF BURYING DEBRIS IS PROHIBITED - VERIFY WITH PARTNER AGENCY (IF USING THIS CLAUSE, DO NOT INCLUDE CLAUSE $$203.05B)*

$$203.05C

203.05(c). Delete the Subsection and substitute the following:

1. **Bury.** Burying debris is prohibited.